**PE08 breaking glass emergency panel:**

**the only one on the market with IP66 protection**

**Thanks its technical features, PE08 breaking glass emergency panel represents the ideal solution to manually activate an emergency signal.**

The AVE innovation in the field of emergency equipment continues. In fact, the **PE08** **breaking glass emergency panel** is the only one on the market with IP66, which ensures maximum **protection against dust and strong water jets**.

Thanks to this feature, **PE08 - IP66** **breaking glass emergency panel is particularly suitable for outdoor installations** - more exposed to atmospheric agents. The typical application is in large buildings, such as thermic power stations, electrical boxes or warehouses, where an emergency supply of this kind is necessary, as well as in the external perimeter of shopping centres and hotels.

In order to meet the needs of the various destination environments, the **PE08 - IP66** **breaking glass emergency panel** also offers the possibility to set the operation for:

* **Automatic start** upon breaking glass (**one action**) by means high profile push button (factory pre-setting);
* **Manual start after** breaking the glass (**two actions**) by means low profile push button included in the supply.

Therefore, the installer can rely on a single model of panel for different applications and decide how to adapt it according to the different installation requirements. There are also **many methods of installation**, with the possibility of **wall mounting** **installation IP66** and **flush mounting installation IP66** via a special box supplied with the panel, or **flush mounting installation IP40** on 2503MG AVE box.

In addition to meet the requirements of product standards EN 60670-1 and EN 60947-5-1, **AVE** **PE08 panel** exhibits technical features that make it **extremely resistant and durable**. Made of high quality plastic material, this device offers a **high shock resistance with IK08** **degree** that allows the maintenance of the IP grade and ensures a **higher longevity**.

Design phase is focused to offer **flexible and reliable products**, but also to ensure **maximum ease of use**for the installers.

**The only one on the market with IP66 protection, PE08 breaking glass emergency panel represents the ideal solution to manually activate an emergency signal**. An innovative device that completes AVE range in this field, which also offers IP55 wall-mounted emergency enclosures, IP40 flush mounted enclosures and flush mounted enclosures for AVE wiring devices.

Rezzato, 14 June 2018

[**www.ave.it**](http://www.ave.it/)